**EGE ÜNİVERSİTESİ**

**MÜHENDİSLİK FAKÜLTESİ**

**BİLGİSAYAR MÜHENDİSLİĞİ BÖLÜMÜ**

**434 GÖRÜNTÜ İŞLEME**

**2019-2020 GÜZ YARIYILI TAKE HOME**

**(Arasınavlardan iki hafta sonraki dersten önce yüklenmeli)**

1. Paint Shop Pro, Photoshop ve GIMP yazılımlarının özelliklerini inceleyiniz ve bu üç yazılımı karşılaştırınız (tablo şeklinde de yazılabilir) [1 sayfa]

Ücretli olanlar internet üzerinden araştırılabilir veya deneme sürümleri indirilebilir. (20 p)

|  |  |  |
| --- | --- | --- |
| **Paintshop Pro** | **Photoshop** | **GIMP** |
| Easier to Learn | High - End Technologies | Free of Use |
| Cheaper | Advanced Layering | Does not Tire Hardware |
| Most Compatible with PC | Most Compatible with Mac | Simple Tools |
| Faster to Learn | SmartPhone Version | Faster to Learn |
| Built-in Tutorials | Slower to Learn | Customizable Interface |
|  | Cloud Storage | Open Source & Modifiable |

1. İki farklı resim bulunuz. Bu resimleri 2 farklı bölütleme (segmentation) yöntemi (threshold, watershed, region growing, split-and-merge, border tracing, …) ile bölütleyiniz. Görüntülerin ilk ve son hallerini rapora ekleyerek, yöntemleri kısaca anlatıp sonuçları yorumlayınız. Görüntülerde kaçar nesne olduğunu saydırınız ve raporda belirtiniz. (20 p)

İpucu : <https://scikit-image.org/docs/dev/api/skimage.segmentation.html>

1. Görüntü İşleme ile ilgili olarak, fotoğraflar üzerinde geçmiş yıllarda düşünüp de yaptıramadığınız çok zor olmayan bir işlemi kısaca anlatınız (Böyle bir şey yoksa, P1 ve take-home’da olmayan bir işlem araştırıp onun üzerinden gidebilirsiniz). Derste öğrendiklerinizle birlikte araştırarak bu işlemi kodlayarak yapmaya çalışınız. İşlem ile ilgili görüntüleri rapora ekleyerek kodlamanın sonucunu yorumlayınız. (20 p)

People often want to hide their impurities from the pictures of themselves. Before the camera beauty filterings started to get popular, filtering photos had been done with using editor programs such as Adobe Photoshop. Using an editor program to process each photo taken takes a lot of time and expertise fort this, camera filterings became quite popular. But there is something these camera filterings cannot do, keeping the natural beauty after the filtering. So i have always thought of such an image processing method that could change minor impurities while not changing any other part of the photo to keep it the most natural looking. My thoughts that only eliminating the red acne scars on the face is enough to make photo beautiful and natural.

There are numerous basic image filtering methods that can be used in combined to achive this filtering.

1. Aşağıdaki kavramları araştırarak kısaca açıklayınız (20 p):

* 1. SIFT (Scale-Invariant Feature Transform)

The **scale-invariant feature transform** (**SIFT**) is a [feature detection](https://en.wikipedia.org/wiki/Feature_detection_(computer_vision)" \o "Feature detection (computer vision)) algorithm in [computer vision](https://en.wikipedia.org/wiki/Computer_vision" \o "Computer vision) to detect and describe local features in images.

SIFT keypoints of objects are first extracted from a set of reference images[[2]](https://en.wikipedia.org/wiki/Scale-invariant_feature_transform" \l "cite_note-Lowe1999-2) and stored in a database. An object is recognized in a new image by individually comparing each feature from the new image to this database and finding candidate matching features based on [Euclidean distance](https://en.wikipedia.org/wiki/Euclidean_distance" \o "Euclidean distance) of their feature vectors. From the full set of matches, subsets of keypoints that agree on the object and its location, scale, and orientation in the new image are identified to filter out good matches. The determination of consistent clusters is performed rapidly by using an efficient [hash table](https://en.wikipedia.org/wiki/Hash_table" \o "Hash table) implementation of the generalised [Hough transform](https://en.wikipedia.org/wiki/Hough_transform" \o "Hough transform). Each cluster of 3 or more features that agree on an object and its pose is then subject to further detailed model verification and subsequently outliers are discarded. Finally the probability that a particular set of features indicates the presence of an object is computed, given the accuracy of fit and number of probable false matches. Object matches that pass all these tests can be identified as correct with high confidence.[[3]](https://en.wikipedia.org/wiki/Scale-invariant_feature_transform#cite_note-Lowe2004-3)

* 1. Corner Detection, Harris Corner Detector

A corner is a point whose local neighborhood stands in two dominant and different edge directions. In other words, a corner can be interpreted as the junction of two edges, where an edge is a sudden change in image brightness.[[3]](https://en.wikipedia.org/wiki/Harris_Corner_Detector#cite_note-derpanis-3) Corners are the important features in the image, and they are generally termed as interest points which are invariant to translation, rotation and illumination. Although corners are only a small percentage of the image, they contain the most important features in restoring image information, and they can be used to minimize the amount of processed data for motion tracking, [image stitching](https://en.wikipedia.org/wiki/Image_stitching" \o "Image stitching), building 2D mosaics, [stereo vision](https://en.wikipedia.org/wiki/Computer_stereo_vision), image representation and other related computer vision areas.

In order to capture the corners from the image, researchers have proposed many different corner detectors including the [Kanade-Lucas-Tomasi](https://en.wikipedia.org/wiki/Kanade%E2%80%93Lucas%E2%80%93Tomasi_feature_tracker" \o "Kanade–Lucas–Tomasi feature tracker) (KLT) operator and the Harris operator which are most simple, efficient and reliable for use in corner detection. These two popular methodologies are both closely associated with and based on the local structure matrix. Compared to the Kanade-Lucas-Tomasi corner detector, the Harris corner detector provides good repeatability under changing illumination and rotation, and therefore, it is more often used in stereo matching and image database retrieval. Although there still exists drawbacks and limitations, the Harris corner detector is still an important and fundamental technique for many computer vision applications.

* 1. Hough Transform

The **Hough transform** is a [feature extraction](https://en.wikipedia.org/wiki/Feature_extraction" \o "Feature extraction) technique used in [image analysis](https://en.wikipedia.org/wiki/Image_analysis" \o "Image analysis), [computer vision](https://en.wikipedia.org/wiki/Computer_vision" \o "Computer vision), and [digital image processing](https://en.wikipedia.org/wiki/Digital_image_processing" \o "Digital image processing).[[1]](https://en.wikipedia.org/wiki/Hough_transform#cite_note-1) The purpose of the technique is to find imperfect instances of objects within a certain class of shapes by a voting procedure. This voting procedure is carried out in a [parameter space](https://en.wikipedia.org/wiki/Parameter_space" \o "Parameter space), from which object candidates are obtained as local maxima in a so-called accumulator space that is explicitly constructed by the algorithm for computing the Hough transform.

1. The classical Hough transform was concerned with the identification of [lines](https://en.wikipedia.org/wiki/Line_(mathematics)" \o "Line (mathematics)) in the image, but later the Hough transform has been extended to identifying positions of arbitrary shapes, most commonly [circles](https://en.wikipedia.org/wiki/Circle" \o "Circle) or [ellipses](https://en.wikipedia.org/wiki/Ellipse" \o "Ellipse).
   1. Laplacian of Gaussian

The Laplacian is a 2-D [isotropic](https://homepages.inf.ed.ac.uk/rbf/HIPR2/isotrop.htm) measure of the 2nd [spatial derivative](https://homepages.inf.ed.ac.uk/rbf/HIPR2/spatdom.htm) of an image. The Laplacian of an image highlights regions of rapid intensity change and is therefore often used for edge detection (see [zero crossing edge detectors](https://homepages.inf.ed.ac.uk/rbf/HIPR2/zeros.htm)). The Laplacian is often applied to an image that has first been smoothed with something approximating a [Gaussian smoothing filter](https://homepages.inf.ed.ac.uk/rbf/HIPR2/gsmooth.htm) in order to reduce its sensitivity to noise, and hence the two variants will be described together here. The operator normally takes a single graylevel image as input and produces another graylevel image as output.

**Rapor (10 p)**

**Özdeğerlendirme tablosu hazırlayarak her bir maddeden kaçar puan alabileceğinizi belirtiniz, varsa hangi maddelerde eksikler olduğunu yazınız. (10 p)** **Raporun sonuna ekleyiniz.**